# Select Input - 10020

Selects Tightening Program withing Source Tightening/Batch within sequence.

Name in SoftPLC: SELECT_INPUT_VALUE

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 1 | 16
TreatZeroAsOne | State | Integer | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE