# Zero Position

This configuration makes a system always return to the original start position for each tightening or sequence. Zero Position is set for each tool separately for both handheld and fixtured. Zero position sets the current position of the tool. It is not possible to set Zero Position during an ongoing tightening or sequence.

Set a zero position:

1. In the home view select Tool.

2. Select Cable Tool and then Zero Position in the right menu.

3. Select SET. The current position of the tool will be set as Zero Position.