# SZP - Set Zero Position

Tools
ES STR SL ST SR QST

The step Set Zero Position sends out the signal set zero position to the tool. The position is repeated once every 360 degrees.

With the steps Loosen to Zero Position or Tighten to Zero Position it is possible to return the tool to zero position.

This step does not have any parameters.

The zero position is a specific position stored with either a “Set Zero Position” step or the signal “Set Zero Position”. The position is repeated once every 360 degrees.