# LST - Low Spot Torque

Tools
ES STR SL ST SR QST IXB

This step monitor measures the lowest torque and checks that it is between the limits.

Parameter | Description
--- | ---
High Limit | Highest acceptable torque.
Low Limit | Lowest acceptable torque.
Type | Specifies the start condition: Step Start: The measurement starts from step start and ends at the shut-off point. Angle Trigger: The measurement starts at the set angle and ends at the shut-off point.
Start Angle | Available when Type is set to Angle Trigger.