# SR - Socket Release

Tools
ES STR SL ST SR QST STB IXB

This step is not supported for tools configured with Gear Front Attachment (GFA) of type open end.

This step runs the tool with speed n in the backward direction until the target angle is reached. The target angle is measured from the start of the step.

This step is only allowed to use as the last step in the tightening path of a multistep tightening program. However, it is possible to add a sync point after this step.

Parameter | Description
--- | ---
Target angle | The angle target. Default: 3 degrees, must be > 0
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Speed ramp | If Speed ramp type is Manual, this field opens. Default: 500 rpm/s.
Speed | Default: 60 rpm.