# TAW - Torque in Angle Window

Tools
ES STR SL ST SR QST STB IXB

This monitor checks that all torque values in the angle window are within the torque limits.

Parameter | Description
--- | ---
Trigger Torque | Must be >= 0
Start Angle | Must be > 0
Window Length | Must be <= 0
Low Limit | Must be >= 0
High Limit | Must be > 0 Must be > Low limit
NOK if window is passed | If set to Yes, status of this monitor is NOK if the end of angle window is not reached.