# A - Angle

Tools
ES STR SL ST SR QST STB IXB MWR-TA

This step monitor measures the maximum angle reached during the monitor and checks that it is between High limit and Low limit.

The angle measurement starts at the start of the monitor or, if specified, at the point where the torque passes Trigger torque for the first time during the monitor.

Parameter | Description | Default value
--- | --- | ---
Stop condition | It specifies where the angle measurement ends: End End point used: the angle at the end of the monitor. Peak Torque End point used: the angle at the point where the highest torque is reached during the monitor. Shut Off End point used: the angle at the shut off point of the step. Peak End point used: the highest angle reached during the monitor. | Shut Off
Trigger torque | The angle measurement starts at this trigger. Minimum limit: must be >= 0 Maximum limit: must be < Tool Max Torque | Not set
Low Limit | Lowest acceptable angle. Minimum limit: must be >= 0 Maximum limit: must be < 9 999 999 and < High Limit | Not set
High Limit | Highest acceptable angle. Minimum limit: Must be > 0 and > Low Limit Maximum limit: must be < 9 999 999 | Not set

## Result Values

- Angle Measured: the angle measured by the monitor.

Point and click on image to see more information:
Step Monitor Angle - Stop condition End

A | Shut-off point | D | Angle high limit
B | Torque trigger | E | Measured angle
C | Angle low limit | F | Step

Point and click on image to see more information:
Step Monitor Angle - Stop condition Peak Torque

A | Peak torque | E | Angle high limit
B | Shut-off point | F | Measured angle
C | Torque trigger | G | Step
D | Angle low limit |  |

Point and click on image to see more information:
Step Monitor Angle, Stop condition Shut Off

A | Shut-off point | D | Angle high limit
B | Torque trigger | E | Measured angle
C | Angle low limit | F | Step

Point and click on image to see more information:
Step Monitor Angle - without Torque Trigger and with stop condition Peak

A | Shut-off point | D | Measured angle
B | Angle low limit | E | Step n-1
C | Angle high limit | F | Step n