# PTCPT - Post Thread Cut Peak Torque

Tools
ES STR SL ST SR QST STB IXB

Measures the maximum torque achieved during the monitoring, including any over-shoot, and checks that it is between the Torque limits. All torque values are ignored until the end of the Thread cut angle window has been reached.

Parameter | Description
--- | ---
Thread cut trigger torque | Must be >= 0
Thread cutting angle window | Must be > 0
Low Limit | Must be >= 0
High Limit | Must be > 0 Must be > Low limit