# Waiting To Continue - 201

Waiting To Continue is an output signal, which means that the tightening has reached a Wait tightening step with the condition Signal configured as Wait Type.
The system (one or more spindles) pauses the tightening waiting for the signal Continue Step - 10128 (for system release) or the sub-signal Channel Command - 10054: Continue Step (for individual spindle release).

For more information, see the sub-signals Bolt Tightening Status - 79: Waiting To Continue and Channel Tightening Status - 80: Waiting To Continue.

Name in SoftPLC: WAITING_FOR_CONTINUE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE