# A - Maximum Angle

Tools
ES STR SL ST SR QST STB IXB

This restriction measures the angle. If the measured angle reaches the Maximum Limit, the tool is stopped immediately. The angle is measured from the start of the restriction or, if specified, from the point where the torque passes Trigger Torque for the first time during the restriction.

Parameter | Description
--- | ---
Trigger Torque | If specified, this is the torque from where the angle is measured.
Maximum Limit | If this limit is reached the tool is stopped immediately.