# A – Tighten to Angle / Loosen to Angle

Tools
ES STR SL ST SR QST STB IXB

A – Tighten to Angle

This step runs the tool until the target angle is reached. The target angle is measured from the start of the step.

A – Loosen to Angle

This step runs the tool with the speed n in the backward direction until the angle target is reached. The target angle is measured from the start of the step.

This step is not supported for tools configured with Gear Front Attachment (GFA) of type open end.

Parameters

Parameter | Description
--- | ---
Target angle | The angle target. Must be > 0.
Speed | Default: 60 rpm.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Speed ramp | If Speed ramp type is Manual, this field opens. Default: 500 rpm/s.
Brake (Valid only for Power Focus 6000 Synchronized tightening, Power Focus 8 Synchronized tightening and Flex). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.

Point and click on image to see more information:

A | Target Angle

## Microvideo

A - Tighten to Angle / Loosen to Angle