# TrR – Loosen to Trigger Release

Tools
ES STR SL ST SR STB IXB

This step is not supported for tools configured with Gear Front Attachment (GFA) of type open end.

This step runs in the backward direction until the tool trigger is released (loosen). It can only be used as a last step in a program.

For STB tools, this step is only applicable for loosening programs.

Parameter | Description
--- | ---
Speed | Numerical value for rotation speed; in rpm.
Speed Ramp Type | List of options where speed ramp can be chosen [Hard, Soft, Manual]