# Configuration of the Tool Alarms

Alarms are set to control when to perform maintenance or calibration on the tools connected to the controller.

The tool service interval and other information are found in the tool view on the Tool menu.

Different tool alarms
Field | Description
--- | ---
Service indicator alarm | Enables an alarm for when the service interval for the tool is reached.
Tool lock after alarm | Lock the tool when the service interval is reached.
Calibration alarm | Enables the tool calibration alarm for all tools connected to the controller.