# Socket Lifted Raw - 10043

Added to support backwards compatibility with PF4000 in certain protocols for socket lifted notifications (as opposed to Socket Lifted 10013). Integer is bit pattern for all lifted sockets (regardless of flashing or how many is lifted).

Name in SoftPLC: SOCKET_LIFTED_RAW

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | uint64 | 1 | 32
SocketSelectorTwoDevices | State | uint64 | 1 | 32

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE