# Cleaning

Keep the MTRwrench clean.

After use, remove any traces of oil and grease from the MTRwrench with a soft cloth and a soft surface cleaner for oil/grease. Do not use aggressive or abrasive cleaner.

Use an anti-static cleaning cloth in order to remove dust from the MTRwrench.

Avoid using harsh detergents to clean the MTRwrench.

Clean the contact of the MTRwrench by using an electrical contact cleaner solution.

## Applies to: