# MTRwrench

# Technical Data

# Environmental Conditions

Indoor use only |
Altitude | Up to 2000 m
Ambient temperature range | +5 to +40 °C (+41 to +104 °F)
Maximum relative humidity 80 % for temperatures up to 31 °C decreasing linearly to 50 % relative humidity at 40 °C |

# Product Data

Operating torque range | from 20% to 100% of the capacity
Torque measurement accuracy (within the operating torque range) | 1%
Mechanical repeatability click | ± 3%
Overload capacity | 150 % of nominal capacity
Maximum angular speed | 250 °/s
Angle measurement accuracy | ± 3.6 ° / 360 ° (at 6 ° per second)
Temperature stability of torque measurement | +10 °C to +40 °C (10 °F to 104 °F)
Tightening results memory capacity | 10000 (maximum)
Power supply | Rechargeable NiMH AA battery 1900mAh 1.2V

# Compatible Battery

A rechargeable NiMH AA battery (1900 mAh, 1.2 V) provides power to the MTRwrench.

The tool is compatible with above mentioned rechargeable batteries.

It is recommended to use the rechargeable batteries with part number
4027 0048 20.

WARNING

Never try to recharge non-rechargeable batteries! Non-rechargeable batteries may leak when charging. They can explode and cause risk of fire and injuries.

# MTRw-Radio Module Frequencies

Refer to the local Regulatory Domain for frequency selection.

## Europe

Number | Channel | Frequency [MHz] | Data rate [bit/s]
--- | --- | --- | ---
1 | 53 | 868.132 | 19200
2 | 54 | 868.176 | 19200
3 | 55 | 868.221 | 19200
4 | 56 | 868.265 | 19200
5 | 57 | 868.309 | 19200
6 | 58 | 868.353 | 19200
7 | 59 | 868.397 | 19200
8 | 60 | 868.442 | 19200
9 | 61 | 868.486 | 19200
10 | 62 | 868.530 | 19200
11 | 63 | 868.744 | 19200
12 | 64 | 868.788 | 19200
13 | 65 | 868.832 | 19200
14 | 66 | 868.876 | 19200
15 | 67 | 868.921 | 19200
16 | 68 | 868.965 | 19200
17 | 69 | 869.009 | 19200
18 | 70 | 869.053 | 19200
19 | 71 | 869.097 | 19200
20 | 72 | 869.142 | 19200
21 | 73 | 869.444 | 19200
22 | 74 | 869.488 | 19200
23 | 75 | 869.532 | 19200

## USA, CANADA

Number | Channel | Frequency [MHz] | Data rate [bit/s]
--- | --- | --- | ---
1 | 1 | 902.132 | 19200
2 | 2 | 902.176 | 19200
3 | 3 | 902.220 | 19200
4 | 4 | 902.264 | 19200
5 | 5 | 902.308 | 19200
6 | 6 | 902.352 | 19200
7 | 7 | 902.396 | 19200
8 | 8 | 902.440 | 19200
9 | 9 | 902.484 | 19200
10 | 10 | 902.528 | 19200
11 | 11 | 902.572 | 19200
12 | 12 | 902.616 | 19200
13 | 13 | 902.660 | 19200
14 | 14 | 902.704 | 19200
15 | 15 | 902.748 | 19200
16 | 16 | 902.792 | 19200
17 | 17 | 902.836 | 19200
18 | 18 | 902.880 | 19200
19 | 19 | 902.924 | 19200
20 | 20 | 902.968 | 19200
21 | 21 | 903.012 | 19200
22 | 22 | 903.056 | 19200
23 | 23 | 903.100 | 19200
24 | 24 | 903.144 | 19200
25 | 25 | 903.188 | 19200
26 | 26 | 903.232 | 19200
27 | 27 | 903.276 | 19200
28 | 28 | 903.320 | 19200
29 | 29 | 903.364 | 19200
30 | 30 | 903.408 | 19200
31 | 31 | 903.452 | 19200
32 | 32 | 903.496 | 19200
33 | 33 | 903.540 | 19200
34 | 34 | 903.584 | 19200
35 | 35 | 903.628 | 19200
36 | 36 | 903.672 | 19200
37 | 37 | 903.716 | 19200
38 | 38 | 903.760 | 19200
39 | 39 | 903.804 | 19200
40 | 40 | 903.848 | 19200
41 | 41 | 903.892 | 19200
42 | 42 | 903.936 | 19200
43 | 43 | 903.980 | 19200
44 | 44 | 904.024 | 19200
45 | 45 | 904.068 | 19200
46 | 46 | 904.112 | 19200
47 | 47 | 904.156 | 19200
48 | 48 | 904.200 | 19200
101 | 101 | 922.552 | 19200
102 | 102 | 922.681 | 19200
103 | 103 | 922.810 | 19200
104 | 104 | 922.939 | 19200
105 | 105 | 923.068 | 19200
106 | 106 | 923.198 | 19200
107 | 107 | 923.327 | 19200
108 | 108 | 923.456 | 19200
109 | 109 | 922.600 | 19200
110 | 110 | 922.800 | 19200
111 | 111 | 923.000 | 19200
112 | 112 | 923.200 | 19200
113 | 113 | 923.400 | 19200
114 | 114 | 923.600 | 19200
115 | 115 | 923.800 | 19200
116 | 116 | 924.000 | 19200
117 | 117 | 924.200 | 19200
118 | 118 | 924.400 | 19200
119 | 119 | 924.600 | 19200
120 | 120 | 924.800 | 19200
121 | 121 | 925.000 | 19200
122 | 122 | 925.200 | 19200
123 | 123 | 925.400 | 19200
124 | 124 | 925.600 | 19200
125 | 125 | 925.800 | 19200
126 | 126 | 926.000 | 19200
127 | 127 | 926.200 | 19200
128 | 128 | 926.400 | 19200
129 | 129 | 926.600 | 19200
130 | 130 | 926.800 | 19200
131 | 131 | 927.000 | 19200
132 | 132 | 927.200 | 19200
133 | 133 | 927.400 | 19200
134 | 134 | 921.390 | 19200
135 | 135 | 921.519 | 19200
136 | 136 | 921.648 | 19200
137 | 137 | 921.777 | 19200
138 | 138 | 921.906 | 19200
139 | 139 | 922.036 | 19200
140 | 140 | 922.165 | 19200
141 | 141 | 922.294 | 19200
142 | 142 | 922.423 | 19200
143 | 143 | 922.552 | 19200
144 | 144 | 922.681 | 19200
145 | 145 | 922.810 | 19200
146 | 146 | 922.939 | 19200
147 | 147 | 923.068 | 19200
148 | 148 | 923.198 | 19200
149 | 149 | 923.327 | 19200
150 | 150 | 923.456 | 19200
151 | 151 | 922.600 | 19200
152 | 152 | 922.800 | 19200
153 | 153 | 923.000 | 19200
154 | 154 | 923.200 | 19200
155 | 155 | 923.400 | 19200
156 | 156 | 923.600 | 19200
157 | 157 | 923.800 | 19200
158 | 158 | 924.000 | 19200
159 | 159 | 924.200 | 19200
160 | 160 | 924.400 | 19200
161 | 161 | 924.600 | 19200
162 | 162 | 924.800 | 19200
163 | 163 | 925.000 | 19200
164 | 164 | 925.200 | 19200
165 | 165 | 925.400 | 19200
166 | 166 | 925.600 | 19200
167 | 167 | 925.800 | 19200
168 | 168 | 926.000 | 19200
169 | 169 | 926.200 | 19200
170 | 170 | 926.400 | 19200
171 | 171 | 926.600 | 19200
172 | 172 | 926.800 | 19200
173 | 173 | 927.000 | 19200
174 | 174 | 927.200 | 19200
175 | 175 | 927.400 | 19200

The MTRwrench uses a sub-band ranging from channel 1 to 48

# 2.4 GHz band channels

Number | Channel | Frequency [MHz]
--- | --- | ---
2011 | 11 | 2405
2012 | 12 | 2410
2013 | 13 | 2415
2014 | 14 | 2420
2015 | 15 | 2425
2016 | 16 | 2430
2017 | 17 | 2435
2018 | 18 | 2440
2019 | 19 | 2445
2020 | 20 | 2450
2021 | 21 | 2455
2022 | 22 | 2460
2023 | 23 | 2465
2024 | 24 | 2470
2025 | 25 | 2475
2026 | 26 | 2480

# Declarations

# Liability

Many events in the operating environment may affect the tightening process and shall require a validation of results. In compliance with applicable standards and/or regulations, we hereby require you to check the installed torque and rotational direction after any event that can influence the tightening result. Examples of such events include but are not limited to:

- initial installation of the tooling system

- change of part batch, bolt, screw batch, tool, software, configuration or environment

- change of air- or electrical connections

- change in line ergonomics, process, quality procedures or practices

- changing of operator

- any other change that influences the result of the tightening process

The check should:

- Ensure that the joint conditions have not changed due to events of influence.

- Be done after initial installation, maintenance or repair of the equipment.

- Occur at least once per shift or at another suitable frequency.

# EU DECLARATION OF CONFORMITY

We, Atlas Copco Industrial Technique AB, SE-105 23 STOCKHOLM SWEDEN, declare under our sole responsibility that the product (with name, type and serial number, see front page) is in conformity with the following Directive(s):
2011/65/EU (RoHS), 2014/53/EU (RED), 2015/863/EU (RoHS amendment)

Harmonized standards applied:
EN 301489-1 V2.2.3; EN 301489-3 V2.3.2; EN 301489-17 V3.2.4; EN 300328 V2.2.2; EN 300220-1 V3.1.1; EN 300220-2 V3.2.1; EN IEC 61326-1:2021; IEC 61326-1:2020; EN 62479:2010

Authorities can request relevant technical information from:
Product Compliance Manager, Atlas Copco Industrial Technique AB, SE-105 23 Stockholm Sweden

Stockholm, 31 January 2025

Lars Eklöf, Managing Director

Signature of issuer

# UK DECLARATION OF CONFORMITY

We, Atlas Copco Industrial Technique AB, SE-105 23 STOCKHOLM SWEDEN, declare under our sole responsibility that the product (with name, type and serial number, see front page) is in conformity with the following UK Regulation(s): S.I. 2017/1206 |
Designated Standards applied: BS EN 301489-1 V2.2.3; BS EN 301489-3 V2.3.2; BS EN 301489-17 V3.2.4; BS EN 300328 V2.2.2; BS EN 300220-1 V3.1.1; BS EN 300220-2 V3.2.1; BS EN IEC 61326-1:2021; BS IEC 61326-1:2020; BS EN 62479:2010 |

Authorities can request relevant technical information from:
Product Compliance Manager, Atlas Copco Industrial Technique AB, SE-105 23 Stockholm Sweden

Stockholm, 31 January 2025

Lars Eklöf, Managing Director

Signature of issuer

Authorised Representative UK
James McAllister, General Manager
Atlas Copco Ltd
Swallowdale Lane
Hemel Hempstead
Hertfordshire HP2 7EA

# WEEE

Information concerning Waste of Electrical and Electronic Equipment (WEEE):
This product and its information, meets the requirements of the WEEE directive/regulations (2012/19/EU), and must be handled in compliance with the directive/regulations.

The product is marked with the following symbol:

Products marked with a crossed-out wheeled bin symbol and a single black bar underneath, contain parts that must be handled in compliance with the WEEE directive/regulations. The entire product, or the WEEE parts, can be sent to your “Customer Center” for handling.

# FCC and ISED Compliance Statement

This device complies with Part 15 of the FCC Rules. Any changes or modifications not expressly approved by the manufacturer could void the user´s authority to operate this device.

Operation is subject to the following two conditions:(1) this device may not cause harmful interference, and (2) this device must accept any interference received, including interference that may cause undesired operation.

The device is only in compliance if no changes or modifications are made to the device.

The device is in compliance with the requirement for RF exposure in the US with 20cm separation distance between the user and the device. The antenna is fixed to the device and no change in antenna or fixation of the antenna is acceptable and such modification is considered to violate the Compliance Statement.

FCC Responsible party:

Name: Rodney Hill

Position: Product Marketing Manager

Address: 3301 Cross Creek Parkway

MI 483 26 Auburn Hills

United States

Mobile: +1 919 272 7837

Email: rodney.hill@us.atlascopco.com

FCC ID: 2AIPFMTR

This equipment has been tested and found to comply with the limits for a Class A digital device, pursuant to part 15 of the FCC Rules. These limits are designed to provide reasonable protection against harmful interference when the equipment is operated in a commercial environment. This equipment generates, uses and can radiate radio frequency energy and, if not installed and used in accordance with the instruction manual, may cause harmful interference to radio communications. Operation of this equipment in a residential area is likely to cause harmful interference in which case the user will be required to correct the interference at his own expense.

ISED Compliance Statement:

This device complies with: CAN ICES-1(A)/NMB-1(A)

(English) This device complies with Industry Canada’s licence-exempt RSSs. Operation is subject to the following two conditions:

(1) This device may not cause interference; and

(2) This device must accept any interference, including interference that may cause undesired operation of the device.

(French) Le présent appareil est conforme aux CNR d’Industrie Canada applicables aux appareils radio exempts de licence. L’exploitation est autorisée aux deux conditions suivantes:

(1) l’appareil ne doit pas produire de brouillage;

(2) l’appareil doit accepter tout brouillage radioélectrique subi, même si le brouillage est susceptible d’en compromettre le fonctionnement.

(English) This equipment complies with RSS102’s radiation exposure limits set forth for an uncontrolled environment under the following conditions:

(1) This equipment should be installed and operated such that a minimum separation distance of 20cm is maintained between the radiator (antenna) and user’s/nearby person’s body at all times.

(2) This transmitter must not be co-located or operating in conjunction with any other antenna or transmitter.

(French) Cet équipement est conforme aux limites d’expositions de la CNR102 applicables pour un environnement non contrôlé aux conditions suivantes:

1) Cet équipement devra être installé et fonctionner de telle manière qu’une distance minimale de séparation de 20cm soit maintenue entre la partie rayonnante (l’antenne) et l’utilisateur / les personnes à proximité à tout moment.

2) Cet émetteur ne doit pas être co-localisé ou opérer en conjonction avec toute autre antenne ou émetteur.

Company Name: Woodstar Inc

Contact Name: Stephane Mercure

Street Address: 46 chemin du Faisan, Saint Sauveur, Quebec, Canada, J0R R1R

Telephone No: 514-667-6868

Fax No: 514-6676870

Email: ms@woodstar.ca

IC_ID: 21556-MTR

# RF Exposure Statement

This portable transmitter has been tested and found to comply with FCC General Population RF Radiation Exposure limits set forth for an uncontrolled environment and meets the FCC radio frequency (RF) Exposure Guidelines. The antenna used for this device must not be co-located or operating in conjunction with any other antenna or transmitter.

# Radio interference

This is a class A product. In a domestic environment this product may cause radio interference.

# Information regarding Article 33 in REACH

The European Regulation (EU) No. 1907/2006 on Registration, Evaluation, Authorization and restriction of Chemicals (REACH) defines among other things requirements related to communication in the supply chain. The information requirement applies also to products containing so called Substances of Very High Concern (the “Candidate List”). On 27 June 2018 lead metal (CAS nr 7439-92-1) was added to the Candidate List.

In accordance with the above this is to inform you that certain electrical components in the product may contain lead metal. This is in compliance with current substance restriction legislation and based on legit exemptions in the RoHS Directive (2011/65/EU). Lead metal will not leak or mutate from the product during normal use and the concentration of lead metal in the complete product is well below the applicable threshold limit. Please consider local requirements on the disposal of lead at product end of life.

# Regional Requirements

WARNING

This product can expose you to chemicals including lead, which is known to the State of California to cause cancer and birth defects or other reproductive harm. For more information go to

https://www.p65warnings.ca.gov/

# Safety

DO NOT DISCARD - GIVE TO USER

WARNING

Read all safety warnings, instructions, illustrations and specifications provided with this power tool.

Failure to follow all instructions listed below may result in electric shock, fire, and/or serious injury.

Save all warnings and instructions for future reference.

WARNING

All locally legislated safety rules regarding installation, operation and maintenance shall be respected at all times.

## Statement of Use

- For professional use only.

- This product and its accessories must not be modified in any way.

- Do not use this product if it has been damaged.

- If the product data or hazard warning signs on the product cease to be legible or become detached, replace without delay.

- The product must only be installed, operated and serviced by qualified personnel in an industrial environment.

In this Section

- Intended Use
- General Power Tool Safety Warnings
- Product Specific Instructions
- Signs and Stickers
- Information on Environmental Labeling of Packaging

# Intended Use

The only recommended use is that specified by the manufacturer.
This product is intended for tightening operations. No other use permitted.

Do not use while charging.

# General Power Tool Safety Warnings

WARNING

Read all safety warnings, instructions, illustrations and specifications provided with this product.

Failure to follow all instructions listed below may result in electric shock, fire, property damage and/or serious injury.

Save all warnings and instructions for future reference.

The term "power tool" in the warnings refers to your mains-operated (corded) power tool or battery-operated (cordless) power tool.

Work area safety

- Keep work area clean and well lit. Cluttered or dark areas invite accidents.

- Do not operate power tools in explosive atmospheres, such as in the presence of flammable liquids, gases or dust. Power tools create sparks which may ignite the dust or fumes.

- Keep children and bystanders away while operating a power tool. Distractions can cause you to lose control.

Electrical safety

- Avoid body contact with earthed or grounded surfaces, such as pipes, radiators, ranges and refrigerators. There is an increased risk of electric shock if your body is earthed or grounded.

- Do not expose power tools to rain or wet conditions. Water entering a power tool will increase the risk of electric shock.

Personal safety

- Stay alert, watch what you are doing and use common sense when operating a power tool. Do not use a power tool while you are tired or under the influence of drugs, alcohol or medication. A moment of inattention while operating power tools may result in serious personal injury.

- Use personal protective equipment. Always wear eye protection. Protective equipment such as dust mask, non-skid safety shoes, hard hat, or hearing protection used for appropriate conditions will reduce personal injuries.

- Prevent unintentional starting. Ensure the switch is in the off-position before connecting to power source and/or battery pack, picking up or carrying the tool. Carrying power tools with your finger on the switch or energising power tools that have the switch on invites accidents.

- Remove any adjusting key or wrench before turning the power tool on. A wrench or a key left attached to a rotating part of the power tool may result in personal injury.

- Do not overreach. Keep proper footing and balance at all times. This enables better control of the power tool in unexpected situations.

- Dress properly. Do not wear loose clothing or jewellery. Keep your hair and clothing away from moving parts. Loose clothes, jewellery or long hair can be caught in moving parts.

- If devices are provided for the connection of dust extraction and collection facilities, ensure these are connected and properly used. Use of dust collection can reduce dust-related hazards.

- Do not let familiarity gained from frequent use of tools allow you to become complacent and ignore tool safety principles. A careless action can cause severe injury within a fraction of a second.

- Hold the power tool by insulated gripping surfaces, when performing an operation where the fastener may contact hidden wiring. Fasteners contacting a "live" wire may make exposed metal parts of the power tool "live" and could give the operator an electric shock.

Power tool use and care

- Do not force the power tool. Use the correct power tool for your application. The correct power tool will do the job better and safer at the rate for which it was designed.

- Do not use the power tool if the switch does not turn it on and off. Any power tool that cannot be controlled with the switch is dangerous and must be repaired.

- Disconnect the plug from the power source and/or the battery pack, if detachable, from the power tool before making any adjustments, changing accessories, or storing power tools. Such preventive safety measures reduce the risk of starting the power tool accidentally.

- Store idle power tools out of the reach of children and do not allow persons unfamiliar with the power tool or these instructions to operate the power tool. Power tools are dangerous in the hands of untrained users.

- Maintain power tools and accessories. Check for misalignment or binding of moving parts, breakage of parts and any other condition that may affect the power tool’s operation. If damaged, have the power tool repaired before use. Many accidents are caused by poorly maintained power tools.

- Keep cutting tools sharp and clean. Properly maintained cutting tools with sharp cutting edges are less likely to bind and are easier to control.

- Use the power tool, accessories and tool bits etc. in accordance with these instructions, taking into account the working conditions and the work to be performed. Use of the power tool for operations different from those intended could result in a hazardous situation.

- Keep handles and grasping surfaces dry, clean and free from oil and grease. Slippery handles and grasping surfaces do not allow for safe handling and control of the tool in unexpected situations.

Battery tool use and care

- Recharge only with the charger specified by the manufacturer. A charger that is suitable for one type of battery pack may create a risk of fire when used with another battery pack.

- Use power tools only with specifically designated battery packs. Use of any other battery packs may create a risk of injury and fire.

- When battery pack is not in use, keep it away from other metal objects, like paper clips, coins, keys, nails, screws or other small metal objects, that can make a connection from one terminal to another. Shorting the battery terminals together may cause burns or a fire.

- Under abusive conditions, liquid may be ejected from the battery; avoid contact. If contact accidentally occurs, flush with water. If liquid contacts eyes, additionally seek medical help. Liquid ejected from the battery may cause irritation or burns.

- Do not use a battery pack or tool that is damaged or modified. Damaged or modified batteries may exhibit unpredictable behaviour resulting in fire, explosion or risk of injury.

- Do not expose a battery pack or tool to fire or excessive temperature. Exposure to fire or temperature above 130 °C may cause explosion.

- Follow all charging instructions and do not charge the battery pack or tool outside the temperature range specified in the instructions. Charging improperly or at temperatures outside the specified range may damage the battery and increase the risk of fire.

Service

- Have your power tool serviced by a qualified repair person using only identical replacement parts. This will ensure that the safety of the power tool is maintained.

- Never service damaged battery packs. Service of battery packs should only be performed by the manufacturer or authorized service providers.

# Product Specific Instructions

# Safety Information

This product is intended for tightening operation and quality control test. No other use permitted. For professional use only.

WARNING

Overloading the wrench can cause structure breaking, which could cause serious injury.

WARNING

Wrong end fitting tools or extensions can cause a sudden wrench release, which could cause serious injury.

WARNING

Never try to recharge non-rechargeable batteries! Non-rechargeable batteries may leak when charging. They can explode and cause risk of fire and injuries.

WARNING

All locally legislated safety rules regarding installation, operation and maintenance shall be respected at all times.

For additional safety information consult:

- Other documents and information packed with this tool

- http://servaidweb.atlascopco.com

- Your employer, union and/or trade association

- http://www.osha.gov (USA)

- http://europe.osha.eu.int (Europe)

# Operation

# Operating the Wrench

Refer to the Product Instructions of MTRwrench.

# Service and Maintenance

# Preventing ESD Problems

The components inside the product and controller are sensitive to electrostatic discharge. To avoid future malfunction, make sure that service and maintenance is carried out in an ESD approved work environment. The figure below shows an example of an appropriate service work station.

# Cleaning

Keep the MTRwrench clean.

After use, remove any traces of oil and grease from the MTRwrench with a soft cloth and a soft surface cleaner for oil/grease. Do not use aggressive or abrasive cleaner.

Use an anti-static cleaning cloth in order to remove dust from the MTRwrench.

Avoid using harsh detergents to clean the MTRwrench.

Clean the contact of the MTRwrench by using an electrical contact cleaner solution.

# Signs and Stickers

The product is fitted with signs and stickers containing important information about personal safety and product maintenance. The signs and stickers shall always be easy to read. New signs and stickers can be ordered by using the spare parts list.

# Information on Environmental Labeling of Packaging

Material | Abbreviation | Numbering
--- | --- | ---
High density polyethylene | HDPE | 2
Polyvinyl chloride | PVC | 3
Low density polyethylene | LDPE | 4
Polypropylene | PP | 5
Polystyrene | PS | 6
Polyurethane | PU | 7
Corrugated fibreboard | PAP | 20
Non-corrugated fibreboard | PAP | 21
Paper | PAP | 22
Wood | FOR | 50
Paper and fibreboard/plastic | C/PAP | 81

EU Decision 129/97/EC.

# Useful Information

# ServAid

ServAid is a portal that is continuously updated and contains Technical Information, such as:

- Regulatory and Safety Information

- Technical Data

- Installation, Operation and Service Instructions

- Spare Parts Lists

- Accessories

- Dimensional Drawings

Please visit: https://servaid.atlascopco.com.

For further Technical Information, please contact your local Atlas Copco representative.

## Applies to: