# Product Data

Operating torque range | from 20% to 100% of the capacity
Torque measurement accuracy (within the operating torque range) | 1%
Mechanical repeatability click | ± 3%
Overload capacity | 150 % of nominal capacity
Maximum angular speed | 250 °/s
Angle measurement accuracy | ± 3.6 ° / 360 ° (at 6 ° per second)
Temperature stability of torque measurement | +10 °C to +40 °C (10 °F to 104 °F)
Tightening results memory capacity | 10000 (maximum)
Power supply | Rechargeable NiMH AA battery 1900mAh 1.2V

## Applies to: