# Exporting All Controller Information

1. On the home view, go to the Controller tab and then select Export/Import on the left pane.

2. Go to the Export window, select the ellipsis icon and then All controller information on the pop-up window.

3. On the Export window, select Export.
   At the end of the exporting process, an exporting pop-up window confirms that the export is completed.
   A PF/IXBExport_<IAM name>_<datetime>.tar.gz file is automatically downloaded.

When exporting All controller information, the controller configuration, the tightening programs, the settings, the results, and the events are exported for further processing. Part of the export is done both from the cable tool and from the connected wireless tools.

All data included in the export is stored in a file "PFExport_<IAM name>_<datetime (lowest value displayed for time is seconds)>.tar.gz", which includes the following files and directories:

- "PFExport_<datetime>_Results.csv": All available results.

  The results are exported in a CSV formatted text file. The latest performed result is the first in the CSV file.

  It is possible to export the following result information for tightenings and loosenings:

Result Information | Tightening Programs | Multistep Programs | Synchronized tightening
--- | --- | --- | ---
Identity number | - | - | X
Type of tightening | X | X | X
Virtual Station name | X | X | X
VIN (Identifier String) | X | X | X
Date and Time | X | X | X
Unique tool identifier | X | X | -
Batch Sequence Name | X | X | -
Batch Sequence Counter | X | X | -
Batch Count | X | X | -
Bolt name | - | - | X
Total status | - | - | X
Total status info | - | - | X
Status | X | X | X
Status info | X | X | X
Mode Name | - | - | X
Tightening program/Multistep Name | X | X | X
Stopping error | - | X | X
Errors | - | X | X
Failing Step | - | X | X
Channel | - | - | X
Target Torque (Nm) | X | X | -
Final Torque (Nm) | X | X | X
Target Angle (deg) | X | X | -
Start Final Angle (Nm) | X | X | X
Final Angle (deg) | X | X | X
Rundown Angle (deg) | X | - | -
Residual torque correlation factor | X | X | -
Elapsed time (s) | - | X | X
Angle low limit (deg) | X | X | X
Angle high limit (deg) | X | X | X
Torque low limit (Nm) | X | X | X
Torque high limit (Nm) | X | X | X
Number of pulses | X | - | -
Current at shutoff (A) | X | X | X
TrueAngle compensation (deg) | X | X | -
Time to rundown complete (ms) | X | - | -
Time to final torque (ms) | X | - | -
Target Text | X | X | -
Step Data | - | X | X
Selftap Torque | X | X | X
Prevailing Torque | X | X | X
Rundown Angle Trigger | X | X | X

The field delimiter and the number format depends on the language settings:

Language | Date/time | Field delimiter | Number format
--- | --- | --- | ---
English (en_US) | MM/dd/yyyy hh:mm:ss | , | 123.456
Czech (cs) | dd.MM.yyyy hh:mm:ss | ; | 123,456
German (de_DE) | dd.MM.yyyy hh:mm:ss | ; | 123,456
Spanish (es_ES) | dd/MM/yyyy hh:mm:ss | ; | 123,456
French (fr_FR) | dd/MM/yyyy hh:mm:ss | ; | 123,456
Korean (ko_KR) | yyyy-MM-dd hh:mm:ss | , | 123.456
Italian (it_IT) | dd/MM/yyyy hh:mm:ss | ; | 123,456
Japanese (ja_JP) | yyyy/MM/dd hh:mm:ss | , | 123.456
Portugese (pt_BR) | Dd/MM/yyyy hh:mm:ss | ; | 123,456
Russian (ru_RU) | dd.MM.yyyy hh:mm:ss | ; | 123,456
Swedish (sv_SE) | yyyy-MM-dd hh:mm:ss | ; | 123,456
Chinese (zh_CN) | yyyy/MM/dd hh:mm:ss | , | 123.456

For synchronized tightening, all available results are in the file named “PFExport_<datetime>_Results.csv.zip”.

- "PFExport_<datetime>_Events.csv": All available events.

  The following event information is exported in a CSV formatted text file:

  - Severity

  - Date

  - Time

  - Code

  - Description

  - Virtual Station that triggered the event (only exported for PF8-Handheld)

  - Carrier (only exported for synchronized tightening)

  - Channel (only exported for synchronized tightening)

- "/settings" - Settings and configurations (used by Import)

For fieldbus exported settings and configurations:

- General Fieldbus configuration (including IP address)

- Fieldbus configuration

- Fieldbus mapping (Virtual station mapping to ProcessDataFrame)

- "jsonConfigurations.zip": Multistep Tightening and Loosening programs are exported as .json files (to be used with MID2500).

- "atlas_sys_d.zip": Logfiles from Drive application.

- "atlas_sys_i.zip": Logfiles from IT application. Only readable by Atlas Copco personnel.

- "atlas_protocol_log.zip": Logfiles from external protocol adapters.

- “ExportInfo.txt”: Text document containing information about the IAM and the Controller.

- "atlas_plc.zip": PLC configuration.

- “licenseInformation.zip”: License Information and System Capabilities.