# Start Tightening Pulse - 10024

The tightening starts at signal. Runs until the tightening is finished, or until the 30 sec timeout in tightening program occurs.

Name in SoftPLC: TIGHTENING_START_PULSE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE