# Configuring the Task Window in a Virtual Station

Selected tasks can either be running a tightening program, running a batch sequence or enabling a task using a source configured in the Sources tab.

Tasks can be monitored from the controller and the result of the tasks can be presented together with any events that may have occurred during the operation.

In this Section

- Assigning a Task to a Virtual Station
- Configuring Manual Mode in a Virtual Station