# Configuring a License Manager

The Atlas Copco license manager is connected to a controller.

Activating the protocol settings on the controller:

1. On the home view, go to the Settings tab and select Server connections on the left pane.

2. On the Atlas Copco License Manager window, configure the following parameters:

   Field | Description
   --- | ---
   On/Off | Enables/Disables communication with the Atlas Copco license manager.
   Server host | Atlas Copco license manager server IP address
   Server port | Atlas Copco license manager server port