# TensorPulse Tightening Stage Parameters

Parameter name | Condition | Description | Default value
--- | --- | --- | ---
Pulse Energy |  | The Pulse energy delivered in the action pulse expressed in a percentage of the maximum energy the tool can deliver in each pulse. | 100%
Reaction force tuning factor |  | The energy delivered by the tool expressed in a percentage value. The reaction force tuning factor is based on the action energy and results in a comfortable reaction. | 40%
Residual torque correlation factor |  | The term Residual torque correlation factor is similar to a calibration and adjusts between the dynamic torque, measured in the electrical tool, and the residual torque, measured by a control tool. | 100%
Premature torque loss detection time |  | A constant increase in torque is assumed when moving from rundown to tightening. A socket slip of, or a broken screw head can cause the torque decrease. This may be detected in a monitoring window. | 200 ms
Target torque |  | Final target torque for the tightening. | 0 Nm
Torque limits |  | Selected by radio buttons. Limits can be Automatically or Manually selected | Manually
Torque min | Torque limits = manual | Minimum torque for the step. | 0 Nm
Torque max | Torque limits = manual | Maximum torque for the step. | 1 Nm
Angle limits |  | Off:Angle limits is turned off. From Rundown complete: Angle limits is turned On. The system starts to monitor the tightening angle as soon as Rundown complete is reached and reports if angle limits are violated. From torque: Rundown angle limits is turned On. The system starts to monitor the tightening angle from the specified torque value and reports if angle limits are violated. | From Rundown complete
Final angle monitoring torque |  | Torque value from where Angle limits monitoring starts. | 20 Nm
Angle min |  | Angle value for lower angle limit from the starting point. | 0°
Angle max |  | Angle value for the upper angle limit from starting point. | 0°
Time min | Time limits = On | Minimum allowed time for tightening. | 10ms
Time max | Time limits = On | Maximum allowed time for tightening. | 1000ms
Pulse limits |  | Selected from a shortcut menu: Off: No pulse limit monitoring. From rundown complete: The monitoring starts when the Rundown complete torque is reached and reports if the number of pulses is outside the limit. From torque: The monitoring starts when the specific torque value is reached and reports if the number of pulses is outside the limit. | Off
Final pulse monitoring torque | Pulse limits = from torque | Torque value from when the pulse limits are monitored. | 18.75 Nm
Pulses min | Pulse limits = on | Minimum number of pulses to reach the final target. | 2
Pulses max | Pulse limits = on | Maximum number of pulses to reach the final target. | 50
Measure angle to | Angle limits = on | Selected from a shortcut menu: Value at peak torque: Measures the angle value at the maximum torque during the tightening. Max angle value: Measures the maximum angle value during the tightening. Value at Shutoff: Measures the angle value before starting the stop stage. | Max angle value