# Machine Capability Test Mode Active - 10148

Machine capability test mode active.

Name in SoftPLC: MACHINE_CAPABILITY_TEST_MODE_ACTIVE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Internal I/O: TRUE

- Stacklight: TRUE

- Operator Panel: TRUE

- User Display: FALSE

- Soft Selector: FALSE

- I/O Expander: TRUE

- Tool LED: TRUE

- Tool Buzzer: TRUE

- Tool Ring: FALSE

- Fieldbus: TRUE

- ST Selector: FALSE

- TLS Tag: FALSE

- Manual Mode: FALSE

- Indicator Box: FALSE

- Tool Vibrator: FALSE

- Automation Rules: TRUE