# Remote Start Configuration

A tightening can be started remotely from an accessory in both single and multiple controller configurations. The switch to activate remote start is found on the connector panel located behind the front access door of the controller.

Whenever using remote start you must enable an emergency stop solution for safety reasons. For more information on emergency stop, see the Product Instructions document for the controller.

When using a tool with some type of safety handle (such as a trigger start button or a safety lever), remote start must be disabled by setting the switch to Off. This is done to ensure that it is not possible to override the safety function within the tool.