# Pin Configurations for Emergency Stop

The controller has an external EM Stop interface and an I/O bus on the connector board that is located behind the front access door.

The pin configuration is different for single controller solutions and for multiple controller solutions. For single controller solutions, the pin configuration depends on whether or not an EM Stop button is connected to the controller.

For more information on pin configurations for Emergency Stop, refer to the Product Instructions document for the controller.