# Stored Results

The controller stores a result for every tightening or loosening performed. The IAM of POWER FOCUS 8 can store up to 100,000 results.

## Showing Stored Results

1. On the home view, go to the Reports tab. Results is automatically selected on the left pane.

2. On the Results window, select View all results.
   The results list shows the following information:

   - Date: date and time of the tightening performed.

   - Virtual Station: Virtual Station which the tightening was performed with.

   - Tightening Program: Tightening Program column shows Multistep Tightening Program name, or Batch Sequence name followed by the Tightening Program name within the Batch Sequence.

   - Result: Torque / Angle result.

   - Limits: Limits column shows values only when the user sets Step Monitor or Step Restriction, or Program Monitor or Program Restrictions.

     Step Monitors, Step Restrictions, Program Monitors and Program Restrictions are applicable for Final Torque and Final Angle.

   - Details: Tightening / loosening result details.

   - Trace checkbox: By selecting a trace checkbox the corresponding result will be shown in the Sync trace result view.

In the Limits column, the minimum / maximum value can be red colored.
In this case, the red colored value means that any of the following has occurred:

- The measured value is lower than the minimum value set in the Multistep Program.

- The measured value is higher than the maximum value set in the Tightening Program.

## Showing and Reading Result Traces

1. On the home view, go to the Reports tab. Results is automatically selected on the left pane.

2. On the Results window, select View all results.
   The results list shows on the Results window.

3. Select the necessary result.
   The tightening trace shows on the Trace Result View window.

The Trace Result View window shows, step by step, the tightening life-cycle.
When the tightening is NOK, the Trace Result View window shows which Step Monitor or Step Restriction has caused it.
On the trace graph, the Step Monitor or Step Restriction that caused the NOK tightening in the Step level, is red colored.

In the upper-right corner of the trace graph, use the left-arrow and the right-arrow to go through the different trace graphs available for the tightening result selected.

The following trace graphs are available:

- Torque / Time

- Torque / Angle

- Angle / Time

- Speed / Time

- Speed / Angle

- Gradient / Time (when the tightening program is configured to make a gradient trace)

- Gradient / Angle (when the tightening program is configured to make a gradient trace)

- Current / Time

- Current / Angle

The start of each step in a multistep program is indicated by a vertical line in the graph.

On the trace graph, it is possible to zoom in and out, move the trace, and read x-axis and y-axis values on a specific point.
On the lower-left corner of the trace graph, select the plus icon (+) to zoom in , the minus icon (-) to zoom out, or the square icon (□) to reset the zoom level back to the default view.

On the lower part of the Trace Result View window, select a step to open a pop-up window with detailed step information.

In this Section

- Viewing Synchronized Traces