# Selected Tightening Program - 69

The actual id of a selected tightening program; 0 if no tightening program selected.

Name in SoftPLC: SELECTED_PSET_ID

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 1 | 16
TreatZeroAsOne | State | Integer | 1 | 16

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: TRUE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE