# Configuring a Wireless Client

1. On the home view, go to the Settings tab and select Network on the left pane.

2. On the Wireless Client window, select Edit.

3. Set Enabled to On.

4. Set DHCP to On or Off depending on the configuration. If set to Off, fill out the required information, provided by the local system administrator:

   - IP address

   - Subnet mask

   - Gateway

5. Enter a Network name (SSID).

6. On the Security window, select Mode and choose a security mode from the list. If WPA2 Personal is chosen, enter a Security key.

7. Enter security parameters and import cert files and keys, as applicable.

8. Edit the Optional Settings as applicable.

9. Select Apply.

   The controller will establish a wireless connection to the network.

10. To access the user interface wirelessly, type the IP address into a web browser.