# Configuration of the Network

The POWER FOCUS 8 can be set up to be accessed from the Atlas Copco software ToolsTalk 2 or from a web browser on a Local Area Network (LAN). It can also be accessed directly from a connected PC. It uses the IPv4 protocol.

The following network interfaces are enabled by default:

Default Network Interfaces
Name | Description
--- | ---
Service port | Interface for service and maintenance personnel
PoE port 1 | Interface to connect additional tools
PoE port 2 | Interface to connect additional tools

The following services are available on the default network interfaces:

- SSH

- Web server interface for system configuration

- DHCP

- Connection of tools

- Retrieve system export files

- Retrieve protocol adapter logs

- NTP (used by tools)

- Product internal interfaces

- Accessory interface

In this Section

- Configuring the Factory Ethernet Port
- Configuring the Bluetooth
- Configuring the channels
- Configuring a Wireless Client
- Configuring the Controller as a Wireless Access Point
- Configuring the Firewall