# Triggering Manual Mode

Manual mode can be activated by a switch or an external system. For example (indicated below), a button on an operator panel can be configured to activate manual mode.

1. On the home view, go to the Configurations tab and select Operator panel on the left pane.

2. If no configuration for an operator panel exists, select the plus icon in the upper-right corner of the screen.

3. On the Configuration window you want to alter, select Edit and then select the ellipsis icon on the position [A,B,C,D,E,F,G,I] to configure.

4. On the Component window, select the ellipsis icon and, on the list, select One way key switch.

5. On the Turn Signal window, select the ellipsis icon and, on the list, select Manual mode (use the arrow buttons to navigate within the list if necessary).

6. Close the Position configuration window.

If the user needs to be notified that Manual mode has been entered or left, then events 4070 and 4071 have to be configured, respectively.