# Assembly Control Mini PN

## Panel PC

# Product Information

# General Information

WARNING

Risk of Property Damage or Severe Injury

Ensure that you read, understand and follow all instructions before operating the tool. Failure to follow all the instructions may result in electric shock, fire, property damage and/or severe bodily injury.

- Read all Safety Information delivered together with the different parts of the system.

- Read all Product Instructions for installation, operation and maintenance of the different parts of the system.

- Read all locally legislated safety regulations regarding the system and parts thereof.

- Save all Safety Information and instructions for future reference.

In this Section

- Safety Signal Words
- Website
- ServAid
- Safety Data Sheets MSDS/SDS
- Country of Origin
- Dimensional Drawings

# Safety Signal Words

The safety signal words Danger, Warning, Caution, and Notice have the following meanings:

DANGER | DANGER indicates a hazardous situation which, if not avoided, will result in death or serious injury.
WARNING | WARNING indicates a hazardous situation which, if not avoided, could result in death or serious injury.
CAUTION | CAUTION, used with the safety alert symbol, indicates a hazardous situation which, if not avoided, could result in minor or moderate injury.
NOTICE | NOTICE is used to address practices not related to personal injury.

# Website

Information concerning our Products, Accessories, Spare Parts and Published Matters can be found on the Atlas Copco website.

Please visit: www.atlascopco.com.

# ServAid

ServAid is a portal that is continuously updated and contains Technical Information, such as:

- Regulatory and Safety Information

- Technical Data

- Installation, Operation and Service Instructions

- Spare Parts Lists

- Accessories

- Dimensional Drawings

Please visit: https://servaid.atlascopco.com.

For further Technical Information, please contact your local Atlas Copco representative.

# Safety Data Sheets MSDS/SDS

The Safety Data Sheets describe the chemical products sold by Atlas Copco.

Please consult the Atlas Copco website for more information www.atlascopco.com/sds.

# Country of Origin

For the Country of Origin, please refer to the information on the product label.

# Dimensional Drawings

Dimensional Drawings can be found either in the Dimensional Drawings Archive, or on ServAid.

Please visit: http://webbox.atlascopco.com/webbox/dimdrw or https://servaid.atlascopco.com.

# Overview

# Applications

The Industrial PC is a computer system which can support several applications, including:

- An interface between the factory network and tightening equipment

- A platform to operate error proofing systems with PC-based visualization

# Technical Data

| Assembly Control Mini PN
--- | ---
CPU Type | Intel® Celeron J6412 @up to 2.60 GHz
Mainboard | ECM-EHL3 A1 J6412 Lite
Mass Storage | 128 GB MLC
Ports | 2x Ethernet 100Mbit/s D coded M12; 2x USB 2.0 Type A; 1x RS232 A coded M12; 2x Profinet 100Mbit/s D coded M12;, 8x I/O (24 V/up to 200 mA, 300mA total) 2 IN, 4 OUT, +/- 24V A coded M12
Display | 10,1": LED TFT, 16:10, 1280 x 800 pixel, brightness typ. 500 cd/m² AUO G101EAN02.2
Touch | PCAP
Ingress Protection | IP54
Type of Battery | 8 Li-Mn02
Operating System | Windows 10 IoT Enterprise LTSC 2021/H2 (standard) Linux (supported) Windows 11 (supported)
Weight (Kg) | 3.5
Weight (lb) | 7.72
Dimensions [L×W×H] (mm) | 48×295.40×213.4
Ambient working temperature (°C) | 0°C to 40°C
Ambient working temperature (°F) | 32°F to 104°F

# External Interfaces

Serial Port | 1×M12 8-pin (male), RS-232 (RS-232/422/485) with waterproof cover and chain
USB Port | 2×Typ A USB 2.0 with waterproof cover and chain
LAN Port | 2×M12 4-pin (female) for LAN with waterproof cover and chain
Power button | 1×Power Switch on the back
Power Connector | 1×M12 4-pin (male) for +24V DC power with waterproof cover and chain

# Position of the S/N label

# Installation

# Installation Requirements

# Primary Interfaces Connections

Ports and external interfaces are present on the back side of the unit. The units ports can be used to connect the Panel PC to an external device.

1 | Profinet 1 | 5 | Power Button | 9 | GPIO Connector
2 | Profinet 2 | 6 | USB 1 | 10 | Power Connector
3 | Ethernet 1 | 7 | USB 2 |  |
4 | Ethernet 2 | 8 | RS-232/422/485 COM |  |

## External I/O Module

GPIO Connector 1x M12 8-pin (female A coded)

GPIO | PIN | Signal Name
--- | --- | ---
| 1 | GND
2 | Out 1
3 | Out 2
4 | Out 3
5 | Out 4
6 | In 1
7 | In 2
8 | 24V

## 1x M12 8-pin (male A coded) RS 232/422/485 COM

(RS-232/422/485 by EMX-APLP)

Serial Port | PIN | RS-232/422/485
--- | --- | ---
| 1 | DCD / 422R+
2 | RXD / 422R-
3 | TXD / 422T- / 485-
4 | DTR / 422T+ / 485+
5 | GND
6 | DSR
7 | RTS
8 | CTS

## 2x M12 4-pin (female D coded) for LAN

2 x M12 4-pin (female) for LAN with waterproof cover and chain

Serial Port | PIN | Pin Define
--- | --- | ---
| 1 | TD+
2 | RD+
3 | TD-
4 | RD-

## Power Connector

1 x M12 4-pin (male coded A) for DC power with waterproof cover and chain

Serial Port | PIN | Pin Define
--- | --- | ---
| 1 | 24V
2 | GND
3 | GND
4 | 24V

# Software Installation Requirements

Installation via any of the following methods is possible:

- PXE boot (network)

- USB stick

- External USB drive

# Power Supply Cable

## Power Supply Cable 100-240 VAC

The product ships with 1xM12 4-pin (female coded A) 24V DC cable. Additionally, the above mentioned cable can be ordered separately. The order number is 8434230421.

If the unit operates with an external power supply, add the cable type with Part Number: 8434230429 to the box. Use one of the following cable types:

4222 1801 13 | Power cable EU - type E/F
4222 1802 13 | Power cable US - type B
4222 1803 13 | Power cable UK - type G
4222 1804 13 | Power cable IN/ZA - type M
4222 1805 13 | Power cable CH - type J
4222 1806 13 | Power cable IT - type L
4222 1807 13 | Power cable AU - type I
4222 1809 13 | Power cable CN - type I
4222 1810 13 | Power cable BR - type N
4222 1811 13 | Power cable IL - type H

WARNING

Risk of electric shock

A not grounded wall outlet may result in electric shock.

- Make sure that the wall outlet is grounded.

# Installation Instructions

# Assembling the Panel PC

- Only qualified personnel shall assemble and operate the Panel PC.

- Only suspended or standing assembly with standard screen of the Panel PC is permitted. Vertical screen orientation is not permitted.

Assemble the Panel PC as follows:

1. Partly install the two bottom screws first. The original size of these screws is 4x M4x10mm with 4x M4 washer included in Part Number 8434230430 AC Mini vesa adapter.

# Connecting the Power Supply Cable

WARNING

Risk of electric shock

A live cable can cause electric shock.

- Make sure that the power cable is not carrying any voltage.

- Switch off the external circuit breaker.

1. Connect the power supply plug (1) to the power connector (2).

2. Connect the power supply cable plug (3) into the mains socket.

3. Switch on the power button (4).

# Operation

# Ergonomic Guidelines

Consider your workstation as you read through this list of general ergonomic guidelines and see if you can identify areas for improvement in posture, component placement, or work environment.

- Take frequent breaks and change work positions frequently.

- Adapt the work area to your needs and the work task.

  - Adjust for convenient reach range by determining where parts or tools should be located to avoid static load.

  - Use workstation equipment such as tables and chairs appropriate for the work task.

- Avoid work positions above shoulder level or with static holding during assembly operations.

  - When working above shoulder level, reduce the load on the static muscles by reducing the weight of the load. You can also reduce the load on the static muscles by holding the load close to the body.

  - Make sure to take frequent breaks.

  - Avoid extreme arm or wrist postures, particularly for operations requiring a degree of force.

- Adjust for convenient field of vision by minimizing movement of the eyes and head during the work task.

- Use the appropriate lighting for the work task.

- Use ear protection equipment in noisy environments.

- Use dust extraction system or mouth protection mask in dusty environments.

# Operating Instructions

# Opening / Closing the Panel PC

Make sure the Panel PC is switched off and the power cord is disconnected.

1. Remove all the screws on the backside of the Panel PC.

2. Carefully lift the back unit of the Panel PC to a maximum 25° to access the internal cabling at the front.

   Be careful not to damage the connectors.

3. Carefully disconnect all cables from the back unit of the panel PC before removing any other parts.

   The connectors, and especially the display connectors, must be handled with care to prevent damage.

4. Put the back unit aside with care not to damage the glass surface.

5. Assemble in reverse order.

6. Put all screws back in position and tighten them lightly.

   Apply the required torque to all screws.

   By opening the housing of Assembly Control Mini (Panel PC), all warranty claims are lost.

# Additional Information

WARNING

Risk of incorrect use

Use of this equipment in not suitable locations may cause risks according to IEC 62368-1 F (F4).

- Make sure that this equipment is not used in locations where children are likely to be present.

The rear surface of the panel PC can become very warm. Be careful when touching the rear surface.

# Turning the Panel PC On and Off

1. Use the On/Off breaker to switch On/Off the computer.

WARNING

Risk of System Damage and failure

Unexpected power loss can cause system damage and failure.

- Do not turn OFF the power button, when the operating system is in use.

# Service

# Preventing ESD Problems

The components inside the product and controller are sensitive to electrostatic discharge. To avoid future malfunction, make sure that service and maintenance is carried out in an ESD approved work environment. The figure below shows an example of an appropriate service work station.

# Replacing the Bios battery

When BIOS buffer battery is replaced, it should be original part type CR2032. Risk of explosion if battery is replaced by an incorrect type. Dispose of used batteries according to the local or regional regulations or instructions.

# Recycling

# Environmental Regulations

When a product has served its purpose it has to be recycled properly. Dismantle the product and recycle the components in accordance with local legislation.

Batteries shall be taken care of by your national battery recovery organization.

# Recycling Instructions

Pos. | Part | Recycle as
--- | --- | ---
1 | Front module | Steel, Glass
2 | Gasket | Rubber
3 | Housing | Steel
4 | Connector Plate | Aluminum
5 | Gasket | Rubber
6 | Cover | Aluminum
7 | Screw | Metal
8 | Screw | Metal
9 | GPIO Connector | Electronics
10 | USB Connector | Electronics
11 | On / Switch | Steel, Electronics
12 | Connector Plate | Steel
13 | Screw | Metal