# Configuration of the Synchronized Tightening

Power Focus S can be configured in two different Synchronized Tightening modes:

- Sync member. This mode is used when the system is connected to a Power Focus 8 through a daisy chain connection. The Power Focus S should be set to Sync member mode, and the Power Focus 8 should be set to Sync reference mode.

- No sync. This mode is used when the system is connected to ToolsControl through the Factory Ethernet port.

## Changing the Mode

1. Go to the Settings tab on the home screen. Select Synchronized Tightening.

2. Select the ellipsis icon (...) on the right. The Choose an item pop-up window opens.

3. Select the preferred mode in the Choose an item pop-up window. Confirm by selecting Apply.

In Sync member mode, the Channel number field will appear. This number sets the channel number of the system when connected to a Power Focus 8.

The system will automatically reboot once the mode change is applied.