# Configuring an ILM Tool Tag

Before configuring an ILM Tool Tag, find all ILM devices.

1. In the Configuration view, on the Tags tab, select the ILM Tool Tag, then select Edit.
   Tag Details pop-up window opens.

2. In the Name box, enter a name for the ILM Tool Tag.

   This step is optional.

3. Choose UWB channel from the UWB Channel drop-down list.

   The ILM Tool Tag must be on the same UWB channel as the ILM Anchors.

   The localization rate can be limited to Restricted 3 Hz.

   This step is optional but can be mandatory to obey regional compliance.

4. Choose position sensitivity from the Filter drop-down list.

5. Close the Tag Details window.

6. In the Configuration view, select Upload Configuration.