# Licenses

Feature licenses are managed through the Functionality Management System (FMS). This allows customers to tailor tool functions to their specific needs through a dynamic licensing scheme.

Licenses can be obtained for individual features or collections of features and can be deployed across multiple virtual stations. The licenses can be returned to the pool when they are no longer required.

Licenses can be downloaded from the Atlas Copco License Portal (ACLP) and managed/distributed through ToolsTalk, or can be stored on a FMS Portable (USB drive) to be inserted into the tool.

Note that the creation and management of a customer account in the ACLP is not covered in this documentation. Contact the local Atlas Copco representative for more information.

There are three types of licenses:

- Virtual Station Type

  A fixed collection of features bundled together in a single package. The Virtual Station Type license determines, among other things, how many programs and sequences can be used, which tightening strategies are available, and the type of reporting that can be done. The features contained in each Virtual Station Type are features that often are used in conjunction with each other, or which have internal dependencies that require the presence of other features in the package. Virtual Station Types licenses are assigned in their entirety to a virtual station. The virtual station can then make use of all features contained in the Virtual Station Type. In order to be able to perform tightenings, a Virtual Station has to be assigned a Virtual Station Type license. Depending on the license type, various tightening options will be enabled or blocked.

- Virtual Station Feature

  Individual features can be purchased as a single licenses to complement the virtual station type licenses.

- Controller Feature

  In order to perform a tightening the Integrated Controller License must be stored on the tool. (Not applicable when the Stand-alone License is assigned to the virtual station.)

There are two classes of licenses available for STRwrench Firmware:

- STRwrench Integrated Controller Production license, which activates the following strategies:

  - Torque.

  - Torque (Control) / Angle (Monitor).

  - Torque (Monitor) / Angle (control).

  - Torque (Control) / Angle (Control) OR.

  - Torque (Control) / Angle (Control) AND.

  - Loose.

  - Yield.

- STRwrench Integrated Controller Quality license, which activates the following strategies:

  - Residual Torque / Angle.

  - Residual Torque / Peak.

It is possible to install one license class as Virtual Station Type and the other one as Virtual Station feature, to activate all the strategies available for STRwrench Firmware.

## License Sources

Licenses used on a tool can be pulled from several different sources. The number of simultaneous sources is limited to 10 (either 10 FMS Portable sources, or one License Server (TT2) in addition to nine FMS Portable sources). If a license is to be added from a source when the source limit (10) has been reached, all licenses from one source need to be removed from the tool to make room for licenses from the other source.

The Source Overview tab (License assignment > Source Overview) provides an overview of the licenses installed on the tool, as well as where they were installed from. A maximum number of 10 different sources can be displayed here, and each will be designated with FMS P (for FMS Portable, or dongle), or License Server (TT2).

Selecting any license source will present that source's detailed license source information. It lists the source name and type, as well as the number and type of licenses in each category (Virtual Station Type, Virtual Station Feature and Controller Feature).

Configuration of features governed by licenses can be done even in the absence of an installed license, for example, configuration of tightening programs. Assigning these features to a tool or virtual station is also possible. However, running the feature without a valid license will require the installation of the appropriate license.

License enforcement is performed at two stages: assignment and runtime (trigger pressed). If a feature for which no license is installed is assigned to a virtual station, a warning message will appear in the tool or task section of the user interface (depending on what is missing). If a feature, for which no license is installed, is started, an event will be presented informing which license is missing. It will not be possible to proceed without a correct license installed. Running an unlicensed feature will, in most cases, result in a locked tool.

## Product Essentials Tutorials

https://www.youtube.com/watch?v=HanD0wI-w9k

In this Section

- Installing Licenses on the Tool
- Removing Licenses from the Tool