# Configuring a Wireless Client

1. Go to Settings in the home menu and select Network in the left pane.

2. Go to Wireless Client and select Edit.

3. Edit the General settings.

   1. Set Enabled to On.

   2. Set DHCP to On or Off, depending on the configuration. If set to Off, ask your local system administrator for the correct settings.

   3. Set the IP address, Subnet mask, and Gateway.

   4. Enter a Network name (SSID).

4. Edit the Security settings.

   1. Select Mode and choose a security mode from the list.

   2. Edit the Security settings as applicable. The available settings depend on which mode is selected.

      Security settings
      Setting | Description
      --- | ---
      Mode | Disabled WPA2 Personal WPA2 Enterprise
      EAP Method | PEAP LEAP TLS TTLS FAST
      Security key | Set the alphanumerical password.
      Identity | Set the identity of the tool.
      User name | Set the user name.
      Password | Set the password.
      CA-cert | Select the CA certificate with the Browse button. It can be either of PEM format or Binary (DER).
      Client-cert | Select the client certificate with the Browse button. It can be either of PEM format or Binary (DER).
      Private key | Select the private key with the Browse button. It can be either of PEM format or Binary (DER).
      Private key password | Set the password used for the private key.
      Fast PAC | Set the Protected Access Credentials (PAC).
      MSCHAPv2 | Set MSCHAPv2 On or Off.
      AES/CCMP | Set AES/CCMP On or Off. If uncertain, set AES/CCMP and TKIP to On and ask your local system administrator for further information.
      TKIP | Set TKIP On or Off. If uncertain, set AES/CCMP and TKIP to On and ask your local system administrator for further information.

5. Edit the Optional Settings as applicable.

   Optional settings
   Setting | Description
   --- | ---
   Hostname | Set a hostname for the tool.
   Warn on signal strength below (dBm) | Set the signal strength at which a warning should be given.
   Roaming threshold (dBm) | Set the signal threshold at which the tool shall connect (roam) to an access point with better signal.
   Active scanning interval (s) | Set the time in seconds between scans when the signal strength is bad, as defined in Roaming threshold (dBm). The tool tries harder to find an access point.
   Passive scanning interval (s) | Set the time in seconds between scans when the signal strength is good, as defined in Roaming threshold (dBm).
   Connect to Hidden Wi-Fi Network | If the network (SSID) is hidden, set this value to On.

6. Select Apply.

   The tool will establish a wireless connection to the network, indicated with the tool's blue connection LED indicator emitting a steady light.

7. To access the user interface wirelessly, type the IP address into a web browser.

## Product Essentials Tutorials

https://www.youtube.com/watch?v=IAhVDKSyFgY