# General Settings

Item | Description
--- | ---
Front LED | On: Front LED is lit when the dedicated button is pressed. Off: Front LED will always be off.
TAG selection | On: Select the Tightening Program/Batch or Batch Sequence according to the TAG number configured in the Batch Sequence/Source Tightening/Source Batch. Off: The tool does not select the Tightening Program/Batch or Batch Sequence.
TAG | On: Information on the TAG is displayed and can be edited in the Integrated Controller Tool > Tool menu. Off: Information on the TAG will not be displayed.
Buzzer | On: Audio signaling device will always be on. Off: Audio signaling device will always be off.
Keyboard source | On: It is possible to select, start and stop tightening programs and batches directly from the tool's EHMI. Off: The EHMI can only be used to navigate the available menus and to acknowledge necessary dialogs on the EHMI screen.
Vibration | On: Vibrating device will always be on. Off: Vibrating device will always be off.
Loose pre-tightening check | On: Accidental unscrewing of an already tightened joint is detected before the tightening starts. Off: Function deactivated.
Smart zeroing | On: If the STRwrench detects any movement during the zero adjustment, the zeroing procedure will start over again. Off: If the STRwrench detects any movement during the zero adjustment, the zeroing procedure will not start over again.
Gauge indicator | On: During the tightening, on the EHMI a gauge indicator gives a visual feedback on the progress of the ongoing tightening. According to the operation's settings, the gauge indicator can display torque progress, angle progress or both. Off: During the tightening, on the EHMI only the numerical values of torque and / or angle are displayed to give a feedback on the progress of the ongoing tightening.