# Configuring a Socket Selector

The Socket Selector is a socket tray with LEDs that assists the operator in selecting the correct socket for the tightening procedure, for example, a batch sequence. When using more than one tightening program, it is convenient to use a selector. When a socket is lifted, the corresponding tightening program is selected.

Several socket selectors can be connected to the virtual station.

To connect the socket selector to the virtual station, go to Integrated Controller Tool > Virtual Station > Accessories and select Choose Accessories.

To set up the socket selector, refer to the Socket Selector Product Instructions.

Configure a socket selector

1. Go to Configurations in the home menu and select Socket selector in the left pane.

2. Issue the configuration with a Name.

3. Select Edit.

4. Select Add or Remove for the correct number of socket slots. Select all the slots that are to be active (indicated in blue).

5. Set Control to External if the socket selection is to be controlled by an external system.

## Product Essentials Tutorials

https://www.youtube.com/watch?v=cmU9pYL-kL4