# AM - Manual Loosen to Angle

This step guides the user in loosening a joint until the target angle is reached. The target angle is measured from the trigger torque.

Parameters

Parameter | Description
--- | ---
Target angle | Angle target value. If Target angle = 0, loosening stops when the torque value goes below the Program starts value.
End cycle time | Starts when the torque goes below the Rundown complete torque after reaching the Target angle. This parameter is not editable.
Ratchet time | Starts when the torque goes below the Rundown complete torque without reaching the Target angle value. This allows the operator to release the torque for a while and recharge during the tightening operation. This parameter is not editable.
Torque correction coefficient | When extensions are used, the wrench measurement might be compensated to show a more accurate torque value. To calculate the correction coefficient, please refer to How to calculate the Torque Correction Coefficient. The parameter is stored in the RFID TAG of the end fitting tool. When extensions are not used, Torque correction coefficient = 1.
Angle correction | When extensions cause additional wrench bending, the wrench angle measurement can be compensated to show a more accurate angle value. To calculate the correction value, please refer to How to Calculate the Angle Correction. The parameter is stored in the RFID TAG of the end fitting tool. When extensions are not used, Angle correction = 0.