# Rundown Parameters

All rundown parameters
Parameter name | Condition | Description | Default value
--- | --- | --- | ---
Self-tap |  | Self-tap is activated through a switch Off: Self-tap is turned off. On: Self-tap is turned on. | Off
Length | Self-tap = On | Defines the angle to turn the socket during Self-tap. Measured from the end of the Start step. | 360°
Speed | Self-tap = On | Defines the speed during Self-tap |
Torque min | Self-tap = On | Torque value for lower Self-tap limit. | 0 Nm
Torque max | Self-tap = On | Torque value for upper Self-tap limit. | Tool max torque
Rundown torque limits |  | Rundown torque limits is activated through a switch Off: Rundown torque limits is turned off. On: Rundown torque limits is turned on. | Off
Offset | Rundown torque limits = On | Angle offset before the Angle interval begins. | 0°
Length | Rundown torque limits = On | Angle defining the Rundown torque limit section. | 360°
Torque min | Rundown torque limits = On | Torque value for lower Rundown torque limit. | 0 Nm
Torque max | Rundown torque limits = On | Torque value for upper Rundown torque limit. | % of target torque
Rundown angle limits |  | Rundown angle limits is selected from a shortcut menu. Off: Rundown angle limits is turned off. From Trigger: Rundown angle limits is turned On. The system starts to monitor the tightening angle as soon as the tool trigger is pressed and reports if angle limits are violated. From torque: Rundown angle limits is turned On. The system starts to monitor the tightening angle from the specified torque value and reports if angle limits are violated. | Off
Rundown angle monitoring torque | Rundown angle monitoring torque = From torque | Torque value from where Rundown angle limits are set |
Angle min | Rundown angle limits = On | Angle value for lower angle limit from starting point | 100°
Angle max | Rundown angle limits = On | Angle value for upper angle limit from starting point | 1000°
Time min | Rundown angle limits = On | Minimum time for the step | 10 ms
Time max | Rundown angle limits = On | Maximum time for the step | 5000 ms
Post view torque |  | Post view torque is activated through a switch Off: Post view torque is turned off. On: Post view torque is turned on. | Off
Torque min | Post view torque = On | Torque value for lower Post view torque limit. |
Torque min offset | Post view torque = On | Angle offset before the Post view torque min interval begins. | 720°
Torque min length | Post view torque = On | Angle length defining the Post view torque min section | 90°
Torque max | Post view torque = On | Torque value for upper Post view torque limit. |
Torque max offset | Post view torque = On | Angle offset before the Post view torque max interval begins. | 360°
Torque max length | Post view torque = On | Angle length defining the Post view torque max section | 90°
Compensate value | Post view torque = On | The Compensate value is selected from a shortcut menu. |
Rundown complete torque |  | Defines the torque value for when snug is reached and the rundown is completed. The program can then move on to tightening the screw. Rundown complete must be less than First torque in multi-step strategies or Target torque in the TurboTight strategy. | 0°