# Configuring Live Result Settings

The Live Result Settings window allows a user to define if Prevailing torque compensation value is shown in live results section of the controller and if prevailing torque compensation value is part of the final torque result or not.

1. Select a controller in the Plant structure .

2. Go to the Configurations tab in the menu bar.

   The workspace area displays the available Configurations.

3. Double-click on an existing General Virtual Station to configure, or select Add to create a new one to configure.

4. In the Live Result Settings window, set the relevant switches to ON or OFF depending on the wanted results.

   If the Show PrT Compensation Value switch is set to ON, the Live Results window in the controller displays the PrT compensation value.

   If the Show Torque with PrT Compensation switch is set to ON, the Live Results window in the controller displays the final torque with the PrT compensation included.

   Setting the switches in the Live Result Settings window to either ON or OFF has no impact unless:

   - The multistep program has a tightening step including a Prevailing Torque step monitor with the Compensation switch set to ON.

   The Live Result window of the controller shows how the results are displayed. Refer to the respective controller User guide for more information on how the results are displayed depending on if Show PrT Compensation Value and Show Torque with PrT Compensation is set to ON or OFF