# Joint Id Result - 31046

Sent together with the results on Fieldbus to indicate which configured Joint Id was used in the specific tightening result. Will not be set until a result where Joint Id is used are performed. It is cleared on next tightening or if any external system request to clear results. If “Read result handshake” is used the Joint Id Result part will clear in accordance to this functionality, as for any other result related results on the Fieldbus. For reading the currently selected Joint Id without a result please se “Activated Joint Id - 225”. For further assistance about setting up Joint Id, see Source Tightening Properties.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | String | 8 | 800

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

- Manual Mode: FALSE

- Indicator Box: FALSE

- Tool Vibrator: FALSE

- Automation Rules: FALSE