# Set CCW Direction - 10132

Set CCW Direction is an input signal which forces the SR21/SL tool to counterclockwise direction.

The SR21/SL tool is forced to counterclockwise direction only if, after being connected with the controller, the signal is set "high".
This operation is essential, even if the signal was set "high" before that the SR21/SL tool was connected with the controller.

If the tool is running clockwise, the signal will switch the direction to counterclockwise.
If the tool is running counterclockwise, the direction will not change.

Set CCW Direction overrides the input signal Toggle CW/CCW For Next Run.

If the signal is set "low", the tool will switch the direction to clockwise.

When the tool is set to counterclockwise, the orange direction LED on the tool lights up.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE