# Current Monitoring

Current monitoring provides extra security to monitor the tightening torque and is a complement to the torque sensor within the tool.

At final target torque, the rotor current is measured and converted to a torque value. If the calculated torque is within 10% of the measured torque, the tightening is considered to be OK.

Current monitoring
Parameter | Description | Default
--- | --- | ---
Current monitoring | Switch with On - Off position Off: Current monitoring is disabled and the tool torque is measured by the torque sensor. On: the current is measured at final torque target and converted to a torque value. The calculated torque is compared to the measured torque. If the difference is within 10%, the tightening is considered to be ok. | Off