# Configuring Manual Mode

Configuration consists of three elements: entering signals, leaving signals and secondary task (note that by primary task is meant the "automatic" task that is assigned to the virtual station under Task). If no secondary task is selected, the primary task will be run.

1. Go to the Virtual station menu, select the virtual station to configure, and then under Manual Mode, select Configure.

2. In the Manual mode configuration screen, set the secondary Task. This determines which task should be run when in manual mode.

   The same tasks (tightening, batch sequence, source) can be set for the secondary task as for the primary task.

3. Set the entering signals to be sent by selecting the Add button.

4. Set the leaving signals to be sent by selecting the Add button.

There is a limit set to 99 signals to be sent for entering and leaving.

The parameters for entering and leaving signals are the same.

Relevant Information

- Pushing Configurations to a Controller
- Triggering Manual Mode