# Output Signal Configuration

An Output Signal can be mapped to a lamp, a stacklight, a siren, a buzzer or a terminal connector. The signal is valid during a programmable duration, or until the next tightening starts.

All the different accessories show where and how an output signal can be mapped.

## Mapping an output signal to a position:

1. Select a component or a position.

2. Select a Signal from the drop-down menu.

3. Set the Duration switch to Time or to Next tightening.

4. If Time is selected, a parameter entry box is displayed. Enter the duration of the output signal in seconds.

5. Set the Pulsating position switch to On for a flashing or intermittent signal, or to Off for a steady signal.

If the position is a stacklight, a Rotating option is also possible.