# Viewing/Editing or Creating a Socket Selector Configuration

The Socket Selector is connected to the I/O and assists the operator in selecting the correct socket for the tightening procedure.

Viewing/Editing a Socket Selector Configuration

1. Select a controller in the Plant Structure .

2. Go to Configurations .

   The workspace area displays a list of created configurations for the selected controller.

3. Double-click on the name of the selected Socket Selector configuration in order to view or edit the configuration.

Creating a Socket Selector Configuration

1. In Configurations , selectAdd.

2. The Create new configuration dialog window is displayed. Choose Socket Selector form the drop-down list, and then select Add.

3. In the Properties area of the menu, enter a configuration name and description.

4. In the Socket Selector Configuration, choose Control type Auto or External.

5. For each socket position that should be active, select the check box .

6. For each socket position that should be inactive, clear the check box.

7. To add or remove a group of four sockets, select either Add or Remove.

Up to 32 socket selector positions can be used.

More information on how a configuration is addressed and assigned to a Virtual Station is given in the Virtual Station section .