# Bolt Tightening Status - 79

Bolt Tightening Status is an output signal that identifies the status for individual bolts in a synchronized tightening. 100 bolts are supported.
Bolt Tightening Status signal shows information related to the running tightening and the result of the last tightening.

Name in SoftPLC: BOLT_TIGHTENING_STATUS

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | uint32 array | 32 | 32
FordResultStatus | State |  | 4 | 4
CompactErrorStatus | State |  | 4 | 4

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

The signal Bolt Tightening Status - 79 contains sub-signals (for more information, see "Output Signals: Sub-signals").

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE