# Handling Loosening Sync Mode Configuration

- Double-click on a loosening Sync Mode to configure that Sync Mode.

Properties
Parameter | Description
--- | ---
Name | A user defined name for the mode.
Description | Description of the mode.

## Bolt Configuration

The bolt configuration of a loosening Sync Mode can only be linked to a loosening multistep program and only lists the available loosening multistep programs.

To add bolt configurations, click ADD or ADD MANY. You can have maximum of 64 bolt configurations.

Parameter | Description
--- | ---
Check box | Used when, for example, deleting a channel.
Channel | Number of the channel, also named drive index.
Loosening program | Select the loosening multistep program defined in the menu Tightening Program.