# Fieldbus parameters for CC Link IE

The table below only lists specific parameters for CC Link IE. For the general parameters, see Fieldbus Parameters General.

Field | Description | Default value
--- | --- | ---
Station number | Each device on the network must be assigned a unique Station Number. |
Network number | The network can be segmented into several parts, each with a unique network number that is used for addressing. |

Relevant Information

- Fieldbus Parameters General
- Fieldbus Parameters General