# Toggle CW/CCW - 10130

Toggle CW/CCW is an input signal which toggles the direction of the SR21/SL tool.
If the tool is running clockwise, the signal will toggle the direction to counterclockwise.
If the tool is running counterclockwise, the signal will toggle the direction to clockwise.

Toggle CW/CCW overrides the input signal Toggle CW/CCW For Next Run.

When the tool is toggled to counterclockwise, the orange direction LED on the tool lights up.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE